# 2c: FP37 Forend
![FP37 Forend Assembly](TopBreak_FP37/Assembly_htmldoc.jpg)

"Flare Projector" 37mm - It's not a weapon.

 * Manual Charging
 * Linear Hammer
 * Single shot
 * Top-break action

<!-- NEW PAGE -->
## Prints
STL Files Location: `Forend/TopBreak_FP37/Prints/`

|ReceiverFront|Forend|BarrelCollar|Extractor|
|-|-|-|-|
|![](TopBreak_FP37/Prints/ReceiverFront_thumb.jpg)|![](TopBreak_FP37/Prints/Forend_thumb.jpg)|![](TopBreak_FP37/Prints/BarrelCollar_thumb.jpg)|![](TopBreak_FP37/Prints/Extractor_thumb.jpg)|

|LatchTab|Cluster|Vertical Foregrip|Sightpost|
|-|-|-|-|
|![](TopBreak_FP37/Prints/LatchTab_thumb.jpg)|![](TopBreak_FP37/Prints/Cluster_thumb.jpg)|![](TopBreak_FP37/Prints/VerticalForegrip_thumb.jpg)|![](TopBreak_FP37/Prints/Sightpost_thumb.jpg)|
<br/>

**These numbers are wrong, TODO: Redo them.** Copied from CAFE12+, ballpark accurate.

| Part              | Filament Used | Print Time @ 0.4mm |
|-------------------|-------------: |------------------: |
| ReceiverFront     | 57g           |   07h17m           |
| Forend            | 189g          | 1d01h10m           |
| BarrelCollar      | 114g          |   15h00m           |
| Extractor         | 14g           |    1h55m           |
| LatchBlock        | 114g          |   15h00m           |
| Cluster           | ?g            |   ?h?m             |
| Vertical Foregrip | ?g            |   ?h?m             |
| **Total**         | 420g          |           2d08h09m |
<br/>

## Vitamins
| Purpose                | Part                             | Quantity |
|------------------------|----------------------------------|----------|
| Extractor Bit          | #2 flat 1/4" Hex Bit             | 1        |
| Extractor Retainer     | 1/4"x1" Dowel Pin                | 1        |
| Extractor Spring       | TODO: 12lb 5/6" OD 2.75" Long    | 1        |
| Latch Bars             | 1/4"x3" Square Rod               | 2        |
| Latch Screws           | #8-32x3/4" Flat Head Screw       | 2        |
| Latch Springs          | (same as sear spring)            | 2        |
| Cluster Bolts          | #8-32x1/2" Flat Head Screw       | 2        |
| Cluster Bolt Nuts      | #8-32x3/4" Heat Set Short        | 2        |
| Foregrip Bolt          | 1/4"-20x3.5" Flat Head Screw     | 1        |
| Foregrip Bolt Nut      | 1/4"-20 Heatset Insert           | 1        |
| Barrel             | 1-5/8-in fence post 18.5" Long       | 1        |
<br/>

### Fence Post Barrel
1-5/8-in x 1-5/8-in W x 8-ft H Silver Galvanized Steel Line Fence Post
Lowes has this stuff for $26/8ft. Item #552282Model #58910128

### Barrel Sleeve
There is no barrel sleeve.


<!-- NEW PAGE -->
## Post-Processing
If you purchased a kit, all the machining is already done for you.

### Foregrip Cluster Heatset
Install the *Foregrip Bolt Nut* on the inside of the *Cluster*.

#### Extractor Slot Machining
File out a 1/4" wide slot in the 6-O'clock position for the extractor bit.
Aim for a 45 degree angle 1/8" deep.

File this same notch in a matching location on the barrel. This is easiest
if you wait until you've installed the *Cluster*.

#### Latch Bars Machining
Drill and tap the the *Latch Rods* 1" from the end -

### Barrel Subassembly
Install the *Barrel* into the *Cluster* and *Foregrip*.
The *Foregrip Bolt Nut* and *Cluster Bolts* should act as set screws to secure
the *Barrel* into the *Barrel Sleeve*.

### Barrel Collar: Extractor Subassembly
1. Insert the *Extractor Bit* into the *Extractor*.
2. Drop the *Extractor Spring* into the *Barrel Collar*'s large rectangular hole.
3. Insert the *Extractor* into the hole, and install the *Extractor Retainer* from the large round hole for the barrel.

### Barrel Collar: Latch Subassembly
1. Insert the *Latch Springs* into the small square holes in the *Barrel Collar*.
2. Insert the *Latch Bars* into the square holes in the *Barrel Collar*.
3. Ensure the *Latch Bars* slide smoothly - file the holes if necessary.
4. Insert the two rectangular tabs of the *Latch* into the underside of the *Barrel Collar
5. Depress the *Latch Bars* while you install the *Latch Screws*.
6. Lube the slots and bars.

### Forend Subassembly
1. Rotate the *Barrel Collar* up into the *Forend*.
2. Install the *Barrel*.
3. Install the *Barrel Collar Screws*
