# Case Hardening Mixture
Charcoal: 6
Salt: 4
Flour: 3

Add water to make paste, form paste around mild steel to be hardened. Enclose in a steel box or clay wrap.

Bake at 1400F and quench in saltwater.

Case depth depends on time.
